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BAU38007D ENTERPRISE SPECIFICATION V10
38 mm Premium Tungsten Carbide Knock-Off Button Bit
Built for Strength. Made to Perform.
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German Engineered Precision for Mining, Quarrying, Tunneling, Construction and Water Well Drilling

Product Overview
━━━━━━
BAUMANN BAU38007D is a 38 mm tungsten carbide knock-off button bit designed for demanding drilling environments. The product combines a heat-treated alloy steel body, premium tungsten carbide buttons, semi-ballistic front geometry and dual flushing holes to support stable penetration, efficient debris removal and reliable performance in abrasive formations.
Features & Benefits
✓ Premium tungsten carbide buttons for superior wear resistance and gauge retention.
✓ Heat-treated alloy steel body for enhanced strength and durability.
✓ Efficient bit geometry for fast penetration and improved drilling productivity.
✓ Suitable for mining, construction, quarrying and water well drilling conditions.
Specifications
	Attribute
	Value

	Diameter
	38 mm

	Part number
	BAU38007D

	Button shape
	Domed / semi-ballistic front

	Button material
	Tungsten Carbide

	Body material
	Heat-treated alloy steel

	Weight (approx.)
	0.45 kg

	Gauge angle
	35 degrees

	Flushing holes
	2

	Application
	Mining, Construction, Quarrying, Water Well Drilling

	Compatible rods
	T38 Thread / 38 mm rods




Actual BAU38007D Product Photos
━━━━━━
Real uploaded BAU38007D product and carton photography included for distributor onboarding, procurement review and product identification.
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Technical Dimension Drawings
━━━━━━
Reference drawing for product communication. Final CAD tolerances must be confirmed against production drawings before manufacturing or tender submission.
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Exploded Bit-Face Diagram
━━━━━━
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Diagram labels major bit-face elements: tungsten carbide gauge buttons, semi-ballistic front buttons, center flushing hole, dual flushing holes and heat-treated alloy steel body.


Performance & Application Positioning
━━━━━━
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Recommended Rock Formations
✓ Granite, basalt, quartzite, dolomite, hard limestone and iron ore formations.
✓ Recommended for abrasive and high-strength formations in mining, quarrying and tunneling environments.
✓ Suggested target range: 80 - 250 MPa UCS, subject to drilling system, operator control and site conditions.


Manufacturing Quality System
━━━━━━
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Quality Assurance
✓ Material selection: alloy steel body and tungsten carbide buttons.
✓ Manufacturing process: CNC machining, heat treatment, button fitment and final inspection.
✓ Recommended enterprise quality framework: ISO 9001:2015, ISO 14001 and ISO 45001 alignment.
✓ Traceability fields: product code, size, batch, inspection date and carton quantity.


Packaging Specification
━━━━━━
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20-Unit Carton / Aluminium Case Option
✓ Standard carton pack quantity: 20 units per master carton.
✓ Industrial box carton for handling and transport.
✓ Optional aluminium carry case for premium distributor presentation or protected site transport.
✓ Product identification: BAU38007D / 38 mm marking.
✓ Packaging supports warehouse storage, distributor handover and site allocation.


Distributor Contact & Commercial Page
━━━━━━
[image: ]
Distributor Positioning
BAUMANN is positioned as a manufacturer-led brand supported by authorized distributors. Public CTA: Find a Distributor.
✓ Find a Distributor
✓ Become a Distributor
✓ Regional technical support and product availability
✓ Product documentation, packaging data and field application support


Procurement-Ready Summary
━━━━━━
Model BAU38007D is specified as a 38 mm knock-off button drill bit with a tungsten carbide cutting system, 7-button configuration, 35-degree gauge angle and dual flushing holes.
Enterprise Positioning Statement
BAUMANN BAU38007D delivers a professional 38 mm drill bit proposition for mining, construction, quarrying and water well drilling applications, supported by actual product photography, technical diagrams, packaging specification and distributor-ready brand material.
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BAUMANN - Superior Drill Bits - German Engineered Precision
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ACTUAL BAU38007D PRODUCT PHOTOS
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TECHNICAL DJMENSION DRAWING
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EXPLODED BIT-FACE DIAGRAM
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PERFORMANCE COMPARISON

Penetration rate High Medium Medium
Service life Long Medium Short
Wear resistance Excellent Good Good
Hole accuracy High Medium Medium
Value for money Excellent Good Fair

Downtime impact Reduced Standard Higher
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PACKAGING ¢ 20 UNIT CARTON / ALUMINIUM CASE
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